**Product Series**

**Titanium and Alloy:**Gr1/Gr2/Gr3/Gr4/Gr5/Gr7/Gr9/Gr11/Gr12/ Gr16/Gr17/Gr18/Gr23   
**Nickel:**N02201/N02200   
**Nickel Alloy:** N04400/N06600/N06601/N08800   
**Zircomium and Alloy:** R60700/R60702/R60704/R60705/R60706

|  |  |  |  |
| --- | --- | --- | --- |
| Name of Product | Size Range | Surface | Standards |
| Bar | Dia：Φ5mm-Φ300mm;  Rect. or sq. cross-sectional area 60mm2 Min.;  Length：300-6000mm; | Lathe smooth,  Grinding polish | ANSI/ASME, DIN, JIS, GB, ISO |
| Seamless Tube and Pipe | OD: Φ12mm-Φ219mm;  Wall：0.5-20.0mm;  Length：1000-12000mm | Pickling  Grinding polish |
| Hot-Rolled Plate | Thickenss：3.0-70.0mm；  Width：300-2500mm;  Length：500-8000mm | Pickling,  Shot blasting,  Grinding |
| Cold-Rolled Plate | Thickness：0.8-6.0mm；  Width：300-1300mm；  Length：500-4000mm | Pickling  Sand blasting |
| Cold-Rolled Strip | Thickness：0.05-3.0mm;  Width：200-1250mm | Pickling  Bright annealing |
| Flange |  | Machining |
| Cake and Ring | OD: Φ150mm-Φ1500mm;  Wall：15-300mm;  Height：20-500mm | Machining |
| Non-Standard Forge Piece | Custom made as customer's request | Machining |
| Pipe Fitting | OD: Φ19mm-Φ1210mm;  Wall：2.0-16.0mm;  including elbow, tee, reducing fittings, etc. | Pickling,  Grinding |
| Fastener |  | Machining |
| Welding Wire | Dia：0.5-6.0mm | Pickling,  Bright annealing |

